Craft Specific Safe Work Practices

**Pipefitter**

* Utilize Fire watch, Fire blanket; Fire Extinguishers were applicable for welding and cutting operations.
* Gas bottles are to be secured to prevent from falling over.
* Eye protection to include either safety glasses or hood as appropriate must be utilized at all times.
* Appropriate gloves must be worn depending on operations. Welding gloves must be worn for welding.
* Ladder safety must be observed.
* Hearing protection must be worn for noisy operations.

**Sheetmetal Worker**

* Eye protection to include either safety glasses or hood as appropriate must be utilized at all times.
* Appropriate gloves must be worn depending on operations.
* Ladder safety must be observed.
* Hearing protection must be worn for noisy operations.
* Sharp metal debris must be cleaned up.
* Hands must remain clear of any cutting blades.

**HVAC Service Technician**

* Eye protection to include either safety glasses or hood as appropriate must be utilized at all times.
* Appropriate gloves must be worn depending on operations.
* Ladder safety must be observed.
* Hearing protection must be worn for noisy operations.
* Lockout- Tagout procedures must be followed.
* Special attention to live electrical circuits must be given.
* No troubleshooting of live electrical circuits with wet clothing (ie: excessive sweat).
* Technician will be careful and aware of body proximity to moving parts.
* Loose clothing will not be worn.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_

Signature Printed Name Date Trade